{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"List1","index":0,"n_rows":63,"n_cols":10,"rows_kept":63,"cut":false,"hidden":false,"merged":[[62,0,62,4]],"flags":["formulas_cached_only"]}
[null,"POPIS DEL ZA REKONSTRUKCIJO OBSTOJEČEGA VODOVODA PLANINA KOBOLI"]
[]
[]
["Zap. št.","Opis del","Količina","Enota","Cena/enoto","Vrednost "]
[null,"PLANINA KOBOLI"]
[]
["I.","PRIPRAVLJALNA DELA"]
[1,"Priprava in organizacija gradbišča pred pričetkom del na trasi (dovoz mehanizacije, ureditev deponij za cevi ter odvečni material,..).",1,"kompl.",0,0]
[2,"Zakoličenje trase obstoječega vodovoda.",140,"m",0,0]
[3,"Zakoličba križanj tras vodovoda z ostalimi komunalnimi vodi.",2,"kos",0,0]
[4,"Izdelava začasne vodovodne prevezave (by-pas) za čas gradnje, s PE 80 cevjo premera 50 mm, 12.5 bar.Potrebna je povezava še 5 priključkov.",1,"kompl.",0,0]
[5,"Obveščanje potrošnikov o motnjah v oskrbi z vodo",1,"kompl.",0,0]
[null,"PRIPRAVLJALNA DELA SKUPAJ",null,null,null,0]
[]
[]
["II.","ZEMELJSKA DELA"]
[1,"Rušenje asfaltnega cestišča debeline 8 cm, s pravilnim odrezom robov, nakladanjem in odvozom na deponijo na razdalji do 5 km.",5,"m2",0,0]
[2,"Rušenje robnikov z vzpostavitvijo v prvotno stanje.",2,"m",0,0]
[3,"Površinski izkopi plodne zemljine (humusa) debeline 20 cm.",100,"m2",0,0]
[4,"Strojni izkopi jarka za vodovod širine 0,6 m do 1,0 m in globine 1,0 do 1,5 m v zemljini IV. kat.",90,"m3",0,0]
[5,"Strojni izkopi jarka za vodovod širine 0,6 m do 1,0 m in globine 1,0 do 1,5 m v zemljini V. kat.",20,"m3",0,0]
[6,"Ročni izkopi okrog obstoječih cevi širine 0,6 m do 1,0 m in globine 1,0 do 1,5 m v zemljini IV. kat.",2,"m3",0,0]
[7,"Planum naravnih temeljnih tal v zemljini III. kat. s točnostjo +- 3 cm po predvidenem naklonu.",85,"m2",0,0]
[8,"Izdelava peščenega nasipa nad cevjo debeline 20 cm iz peska granulacije 0-16 mm. ",17,"m3",0,0]
[9,"Strojno zasipavanje jarka pod asfaltnim cestiščem s tamponom 0-30mm. Zasip je treba nabijati v plasteh po 30 cm. ",3,"m3",0,0]
[10,"Zasipanje jarka z izkopanim materialom - strojno nabijanje v plasteh do 30 cm.",44,"m3",0,0]
[11,"Nakladanje, odvoz in razkladanje odvečnega materiala na deponijo do 5 km.",20,"m3",0,0]
[12,"Razrez in dstranjevanje obstoječih PE HD cevi DN 110 mm ter odvoz na deponijo komunalnih odpadkov.",140,"m",0,0]
[13,"Priprava in krpanje z asfaltom granulacije do 11 v debelini 8 cm",5,"m2",0,0]
[14,"Humuziranje travnika debelini 20 cm z valjanjem.",100,"m2",0,0]
[15,"Zatravitev in gnojenje",100,"m2",0,0]
[16,"Izdelava geodetskega posnetka in vnos v kataster komunalnih vodov.",140,"m",0,0]
[null,"ZEMELJSKA DELA SKUPAJ",null,null,null,0]
[]
[]
["IV.","MONTAŽNA DELA IN VODOVODNI MATERIAL"]
[]
[null,"OPOMBA: Vsa vodovodna armatura, fazonski kosi in cevi morajo biti izdelani za pritiske do 16 bar. "]
[1,"Dobava, montaža in tesnenje cevi iz nodularne litine DN 100 in s standardnim tesnilom.",140,"m",0,0]
[2,"Dobava, montaža in tesnenje FF kosa, l=500 mm, DN 100 mm.",1,"kos",0,0]
[3,"Dobava, montaža in tesnenje FF kosa, l=800 mm, DN 100 mm.",1,"kos",0,0]
[4,"Dobava, montaža in tesnenje MMK 11 kosa, DN 100 mm,",2,"kos",0,0]
[5,"Dobava, montaža in tesnenje MMK 22 kosa, DN100 mm.",2,"kos",0,0]
[6,"Dobava, montaža in tesnenje E kosa, DN 100 mm.",4,"kos",0,0]
[7,"Dobava, montaža in tesnenje F kosa, DN 100 mm.",2,"kos",0,0]
[8,"Dobava, montaža in tesnenje T kosa, DN 100/100 mm.",1,"kos",0,0]
[9,"Dobava, montaža in tesnenje T kosa, DN 100/80 mm.",1,"kos",0,0]
[10,"Dobava, montaža in tesnenje Q kosa DN 80 mm.",1,"kos",0,0]
[11,"Dobava, montaža in tesnenje slepe prirobnice (X kos) DN 100 mm.",1,"kos",0,0]
[12,"Dobava, montaža in tesnenje EURO zasuna, z vgradno armaturo in cestno kapo, DN 100 mm, tip 23 PN 16.",2,"kos",0,0]
[13,"Dobava, montaža in tesnenje univerzalnega navrtnega zasuna 1\" za cev DN 100.",5,"kos",0,0]
[14,"Dobava, montaža ter ustrezna izolacija spojev z dekorodalom in plastizoloin pocinkanih cevi s trdo PVC izolacijo.",18,"m",0,0]
[15,"Dobava, montaža in tesnenje podtalnega hidranta DN 80 mm, komplet s cestno kapo.",1,"kos",0,0]
[16,"Dobava, montaža in tesnenje N kosa, DN 80 mm.",1,"kos",0,0]
[17,"Dobava, montaža in tesnenje priključne MS spojke 1\"/32",5,"kos",0,0]
[18,"Dobava, montaža univerzalne enojne spojke za cev DN 100 s tesnenjem",2,"kos",0,0]
[19,"Izdelava in namestitev prefabriciranih  podložnih plošč za hidrante, zasune, odcepe in cestne kape.",2,"kos",0,0]
[20,"Tlačni preizkus",140,"m",0,0]
[21,"Izpiranje sistema ter dezinfekcija",140,"m",0,0]
[22,"Blindiranje obstoječih cevi; ocena.",2,"kos",0,0]
[null,"MONTAŽNA DELA IN VODOVODNI MATERIAL SKUPAJ",null,null,null,0,null,null,null," "]
[]
["Gradbena in Strojnoinstalacijska dela skupaj  v Eur",{"$nulls":4},0]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}