{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["A.01"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":1,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"A.01","index":0,"n_rows":65,"n_cols":12,"rows_kept":65,"cut":false,"hidden":false,"merged":[[54,2,54,7],[33,2,33,7],[46,2,46,7],[58,2,58,7],[9,2,9,7],[13,2,13,7],[42,2,42,7],[50,2,50,7],[29,2,29,7],[17,2,17,7],[38,2,38,7],[21,2,21,7],[25,2,25,7]],"flags":["formulas_cached_only"]}
[null,"0","SKRITO",{"$nulls":8},0]
[]
[null,null,"Objekt: ","Ureditev okolice za avtobusno postajo in ob objektu stare šole v Batujah "]
[]
[null,null,"Investitor: Občina Ajdovščina"]
[]
["SKRITO",null,"Popis del:",{"$nulls":6},"Cena",null,"Znesek   EUR"]
[]
[1,1,"Ureditev in zavarovanje gradbišča"]
[null,null,"Ureditev in zavarovanje gradbišča - ocena."]
[{"$nulls":4},"KOM",null,1]
[]
[1,2,"Izkop zemeljskega platoja"]
[null,null,"Strojni delno ročni površinski izkop v terenu III. ktg. v območju ureditve platojev z nakladanjem in odvozom v stalno deponijo na razdalji do 5 km."]
[{"$nulls":4},"M3",null,60]
[]
[1,3,"Planiranje dna izkopa"]
[null,null,"Planiranje dna celotnega izkopa z utrditvijo in nabijanjem."]
[{"$nulls":4},"M2",null,500]
[]
[1,4,"Tamponsko nasutje"]
[null,null,"Dobava in vgradnja kamnitega tamponskega materiala v deb. do 30 cm s finim planiranjrm planiranjem in uvaljanjem do potrebne nosilnosti."]
[{"$nulls":4},"M3",null,60]
[]
[1,5,"Vrtni robniki 8/20 cm"]
[null,null,"Dobava in polaganje vrtnih robnikov dim. 8/20 cm skupaj s podložnim betonom, obbetoniranjem in fugiranjem (položeni ravno in v krivini) - (izkop s planiranjem in utrditvijo terena zajet v prejšnjih postavkah) - vrtni robniki asfaltnega pločnika mejnih linij tlakov."]
[{"$nulls":4},"M1",null,70]
[]
[1,6,"AB podporni zid; h=cca 100 cm"]
[null,null,"Izvedba AB podpornega zidu višine do 100 cm, na mestu obstoječega delno porušenega ob objektu avtobucne postaje: komplet s temeljem dim. 80/40 in AB zidom višine 100 cm deb. 30 cm (MB 30), z armaturo in opaži - obračun po m1 zidu (izkop s planiranjem in utditvijo zajet v prejšnjih postavkah)."]
[{"$nulls":4},"M1",null,10]
[]
[1,7,"Podložni beton"]
[null,null,"Dobava in vgradnja podložnega betona deb. 8 cm z minimalno armaturo na že izvedeno tamponsko nasutje - za polaganje pranih plošč."]
[{"$nulls":4},"M2",null,35]
[]
[]
[1,8,"Prane plošče"]
[null,null,"Dobava in polaganje prnih plošč dim 40/40/4 cm na cementni estrih komplet s fugiranjem s fino cementno malto skupja z vsemi potrebnimi deli. "]
[{"$nulls":4},"M2",null,35]
[]
[1,9,"Asfaltacija parkirišč - BB-11 deb. 6 cm"]
[null,null,"Asfaltacija parkirišč - BB11 v deb. 6 cm komplet z izvedbo spojev - strojno, delno ročno."]
[{"$nulls":4},"M2",null,500]
[]
[1,10,"Asfaltacija pločnika - BB-08 deb. 4 cm"]
[null,null,"Asfaltacija pločnika - BB08 v deb. 4 cm komplet z izvedbo spojev."]
[{"$nulls":4},"M2",null,40]
[]
[1,11,"Humusiranje zelenic in zatravitev"]
[null,null,"Dobava in planiranje humusa v deb. cca 30 cm."]
[{"$nulls":4},"M2",null,30]
[]
[1,12,"Črtanje asfaltnih parkirišč"]
[null,null,"Črtanje asfaltnih parkirišč v beli barvi deb. 10 cm s predhodnim zarisovanjem."]
[{"$nulls":4},"M1",null,50]
[]
[1,13,"Nepredvidena dela"]
[null,null,"Nepredvidena dela - z vpisom v gradbeni dnevnik in potrditvijo nadzornega organa - predvidi se 5%  od vseh del."]
[{"$nulls":4},"KOM",null,1]
[]
["SKRITO",null,"Skupaj EUR:"]
[{"$nulls":4},"DDV 20%"]
[]
[1,null,"Skupaj z DDV:"]